[INSERT PLANNING SCHEME NAME] PLANNING SCHEME
MODERATE FLOOD RISK SCHEDULE [NUMBER] TO CLAUSE 44.09 FLOOD MANAGEMENT OVERLAY19/10/2026

Shown on the planning scheme map as FMO[number].
NAME OF SCHEDULE
Purpose
To identify land at moderate flood risk (riverine, coastal and overland flows from stormwater) within the 1 per cent Annual Exceedance Probability (1 in 100 year) flood extent.
1.0 Flood management objectives to be achieved19/10/2026

Where no objectives are specified insert “None specified.”
or
Clause 44.09 specifies a schedule may contain flood management objectives to be achieved. Insert a maximum of 5 objectives.
2.0 Statement of risk19/10/2026

Land in this overlay is subject to moderate flood risk. Flooding can affect the safety of people and vehicles.
Floodwater can be difficult to see through and may obscure hazards, including debris and damage to road surfaces. Conditions can change during an event, including rising water levels and reduced warning time.
Floodwater can:
· Cover roads, traffic routes and low-lying areas.
· Reduce vehicle control and stability.
· Disrupt safe access to and from properties.
· Isolate properties.
Flooding has the potential to impact:
· Public safety.
· Buildings, property and other assets.
· Emergency services and essential infrastructure.
· Community infrastructure and services.
· Public health through contaminated floodwater.
· The natural environment.
· Economic wellbeing and social cohesion of communities.
· Cultural heritage values and places.
Clause 44.09 specifies a schedule may contain a statement of risk. Insert any additional statement of risk content.
3.0 Requirement19/10/2026

Use of land
A permit is required to use land for:
· Accommodation (other than dwelling and small second dwelling).
· Art and craft centre.
· Cemetery.
· Crematorium.
· Education centre.
· Emergency services facility.
· Freeway service station.
· Funeral parlour.
· Hospital.
· Indoor recreation facility.
· Industry.
· Intensive animal production.
· Motor racing track.
· Office.
· Pig farm.
· Poultry farm.
· Poultry hatchery.
· Place of assembly.
· Retail premises.
· Service station.
· Reservoir.
· Warehouse.
Any use listed in clause 62.01 if the corresponding requirement in clause 62.01 is not met.
Building and works
A permit is required to construct a building or construct or carry out works, including:
· A fence.
· Roadworks.
· Bicycle pathways and trails.
· A domestic swimming pool or spa and associated mechanical and safety equipment if associated with one dwelling on a lot.
· A domestic rainwater tank with a capacity of more than 4,500 litres.
· A non-domestic rainwater tank with a capacity of more than 10,000 litres.
· A pergola or verandah, including an open-sided pergola or verandah to a dwelling or small second dwelling with a finished floor level not more than 800mm above ground level and a maximum building height of 3 metres above ground level.
· A deck, including a deck to a dwelling with a finished floor level not more than 800mm above ground level.
· A disabled access ramp.
A permit is not required to construct a building or construct or carry out works for:
· Roadworks, tramway, railway or bicycle paths and trails if any of the following apply:
· The water flow path is not redirected or obstructed.
· The roadworks, tramway, railway or bicycle paths and trails are constructed or carried out by or on behalf of the municipal council, public authority or the Head, Transport for Victoria, to the satisfaction of the relevant floodplain management authority.
· Flood mitigation works carried out by or on behalf of the floodplain management authority, municipal council, public authority or the Head, Transport for Victoria.
· An open-sided building associated with grazing animal production constructed on the same land or contiguous land in the same ownership.
· The following works carried out to the satisfaction of the responsible authority:
· The laying of underground sewerage, water and gas mains, oil pipelines, underground telephone lines and underground power lines provided they do not alter the topography of the land.
· The erection of telephone or power lines provided they do not involve the construction of towers or poles designed to operate at more than 66,000 volts.
· Landscaping, driveways, vehicle crossovers, footpaths or bicycle paths if there is no significant change to existing surface levels or if the relevant floodplain management authority has agreed in writing that the flow path is not obstructed.
· An extension of less than 20 square metres in floor area to an existing building (not including an outbuilding).
· Alterations and additions to an upper storey of an existing building.
· An alteration to an existing building where the original building footprint remains the same and floor levels are constructed to at least 300mm above flood level.
· An outbuilding (including replacement of an existing building) if the outbuilding is less than 10 square metres in floor area and constructed to at least 150mm above the flood level or the relevant floodplain management authority has agreed in writing that the flow path is not obstructed.
· A replacement building (not including an outbuilding) if it is constructed to the Nominal Flood Protection Level as determined by the relevant floodplain management authority and the original building footprint remains the same. The responsible authority may require evidence of the existing building envelope.
· A fence with at least 25% openings.
· A replacement fence in the same location and of the same type and materials as the existing fence.
· A pergola or an open deck area with unenclosed foundations.
· A carport constructed over an existing car space.
· An in-ground swimming pool and associated security fencing, where the perimeter edging of the pool is constructed at natural surface levels and excavated material is removed from the flow path.
· A tennis court at existing surface level with fencing designed to minimise obstruction to flows.
· An aviary or other enclosure for a domestic animal if it is less than 10 square metres in floor area at ground level.
· An open-sided verandah, open-sided picnic shelter, barbeque and park furniture (excluding playground equipment) if there is less than 30mm change to existing surface levels.
· A radio mast, light pole or a sign on a post or attached to a building.
· Buildings and works associated with agriculture constructed or carried out to the satisfaction of the relevant floodplain management authority.
Subdivision
A permit is required to subdivide land.
Local floodplain development plan
Name of plan incorporated into this scheme
An application must be consistent with the local floodplain development plan that applies to the land.
4.0 Application requirements19/10/2026

An application must be accompanied by the following information as appropriate:
· The boundaries and dimensions of the site.
· Relevant existing and proposed ground levels to Australian Height Datum, taken by or under the direction or supervision of a licensed land surveyor.
· The layout, size and use of existing and proposed buildings and works, including vehicle parking areas, entry and exit points and basement ramps.
· Floor levels of existing and proposed buildings to Australian Height Datum including vehicle parking areas, entry and exit points and basement ramps.
· The proposed building entry and exit points and basement ramps and ground levels along access and egress routes within the property boundary to Australian Height Datum including cross sectional details of any basement entry ramps and other basement entries to Australian Height Datum, showing floor levels of entry and exit areas and drainage details.
· The 1 per cent Annual Exceedance Probability (1 in 100 year) flood extent and the Nominal Flood Protection Level, as determined by the relevant floodplain management authority.
· The 1 per cent Annual Exceedance Probability (1 in 100 year) flood level showing the proposed ground and finished floor level and the Nominal Flood Protection Level, as determined by the relevant floodplain management authority.
· The location of overland flow paths in relation to proposed buildings and works and flow paths for the passage of overland flows to Australian Height Datum.
5.0 Decision guidelines19/10/2026

Before deciding on an application, in addition to the decision guidelines in clause 65, the responsible authority must consider, as appropriate:
· Whether the proposed use or development could be located on flood-free land or land with a lesser flood risk not affected by this schedule.
· The susceptibility of the development to flooding and flood damage.
· Flood risk factors to consider include:
· The frequency, duration, extent, depth and velocity of flooding of the site and accessway.
· The flood warning time available.
· The danger to the occupants of the development, other floodplain residents and emergency personnel if the site or accessway is flooded.
· The potential to isolate land not at risk of flooding from safe access within or outside this overlay.
· The effect of the development on redirecting or obstructing floodwater, stormwater or drainage water and the effect of the development on reducing flood storage and increasing flood levels and flow velocities.
· The likely or modelled extent of any impact of the development on floodwaters, including the nature and extent of impact on surrounding properties.
· Whether any proposed strategies to minimise or mitigate risk of flood damage or safety will be effective over the life of the development.
· Whether the proposed development maintains existing flood storage capacity and flow paths and conveyance.
· Whether the proposal appropriately responds to the identified site-specific flood risk and the availability of a safe, practical and viable evacuation.
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